### MP-184 Probe changer overtravel error

The CMM has approached a station incorrectly when loading or unloading a probe.

What you should do

1. To clear the error, click Clear error in the XYZ Display window. To clear it using an RCU-II, press and hold down the Servo Power Off button and then press the Joy button twice.

2. Recalibrate the automatic probe changer (APC) rack.

3. Recalibrate the stations.