#### Move Speed %

The Move Speed box lets you change the point to point positioning speed of the CMM. The value that is entered is a percentage of the maximum machine speed. It can be set to any value between 1 and 100% of full machine speed. (See the "Measure" topic under "Defining Probes" in the "Defining Hardware" section for information regarding the move speed option and probe calibration.)

The Edit window command line for this option reads:
MOVESPEED/ nnn.nnnn