### Center Point and Radius (for Rotary Scan)

The X, Y, and Z values of Center define the center point of the ROTARY scan.

You can directly type the center point X, Y, and Z values or you can choose the Select Center check box and click on the CAD drawing to take the center point directly from the CAD model.

R defines the radius. When PC-DMIS executes the scan it will rotate around the center point maintaining this distance as the scan moves from the Start to the End point.