### BF - Turn Soft Probe Off

The BF command disables the soft probe. If a three-axis analog probe (e.g., the Renishaw SP-600) is in use, then the touch probe is enabled.

Command Format

MLString "BF"

Example

1. MLString "BF"

Input

None.

Results

The system disables the soft probe and stops including soft probe deflections as part of the tip position coordinate data.

Skip Action

Ignored.

Error Messages

None.