### MP-698 E-stop circuit open

The emergency stop (E-stop) circuit was open at power up.

Refer to DCC Error Codes for additional information.

What you should do

1. Some systems have console E-stop buttons that lock when pressed. If locked, twist knob clockwise to release.

2. To clear the error, power MP down.

3. Power MP back up.

4. Check all E-stop buttons and the circuit to see if any are open.

5. If the error reoccurs, call your Giddings & Lewis service representative.