### LKRS232 Interface

The LKRS232 interface is used with eight different LK controllers: Cupe Serial, Cupe GPIB, Micron Drive, LK3000, LK2000/2002/2000+, LK4000, the ACT, and the AIM. The LK-3000 is older than both the LK-2000 and the LK-4000. The ACT is the replacement for the 2000 line and the AIM is the replacement for the 4000.

Before starting PC-DMIS, rename the lkrs232.dll to interfac.dll.

The Machine Option dialog box has seven tabs for the LKRS232 interface:

LK Direct tab

See the "LK Direct tab" topic.

Controller tab

See the "Setting the Communication Protocol" topic. Default value is Comm Port 1, 9600 Baud, No parity, 8 data bits, and 1 stop bit.

Axis tab

See the "Assigning the Machine Axes" topic.

Resolution tab

See the "Setting the Axes Scale Factor" topic. Default is X=10000.000000, Y=10000.000000, Z=10000.000000.

Rotary tab

See the "Rotary Table Settings" topic. Default values are: Acceleration = 0.0, Velocity = 0.0, Resolution = 10000, Offset = 0.000000, Offset 2 = 0.000000, Min delta = 0.5, Table = Unchecked, and Dual table = Unchecked.

Debug tab

See the "Generating a Debug File" topic.

Note: Additional information for this interface is provided in the Machine Interface Installation Manual (MIIM).