### IL - Initialize Library

The IL command initializes the Measurement Library. Flags and variables revert to the default state at system initialization. This function does not clear system errors caused by a fault in the system hardware. Separate corrective action must be taken for such errors.

Command Format

MLString "IL"

Examples

1. MLString "IL"

Input

None.

Results

The system:

- Deletes all measured features,

- Resets the part and machine scale ratios to 1:1,

- Cancels axis translations and rotations,

- Sets the feature number and sequence number to zero,

- Reverts to the default values for measurement units and the working plane, and

- Clears all other variables or sets them to the default values.

This function does not affect:

- Selected tip or Probe diameter,

- Calibration of any probe tips,

- Calibration of the rotary table, or

- Saved reference frames 1 through 48. Other reference frames are deleted

Skip Action

This function may not occur in a section of code to be skipped. Error.

Error Messages

None.