### Constructing a Parallel Line

A line can be constructed parallel to any two features. PC-DMIS creates a line parallel to the first input feature and passing through the center of the second input feature.

To construct a Parallel Line:

1. Access the Construct Line dialog box (Insert | Feature | Constructed | Line).

2. Select the Parallel option.

3. Select two features of any type.

4. Click the Create button.

5. The Edit window command line for this option would read:
   CONSTR/LINE,PLTO,feat_1,feat_2,
   length

Constructing a Parallel Line | A - Line constructed parallel to the first feature and through the second feature. B - First feature C - Second feature D - FRONT