### Option 1

In the Probe Utilities dialog box, select the Add Angles option. This will allow you to key in new A,B angle pairs to the probe file. If the tip has already been calibrated, then the new A,B combinations will also be calibrated and ready to use. Once you leave the Probe Utilities dialog box, you can use these new A,B combinations by selecting them from the Tip List box located on the toolbar.