Current Help System: PC-DMIS CMM (View Core Help)

#### Axis Basic Scan - Surface Data Method

To generate a line using surface data:

1. Click the Surface mode icon.

2. Select Start Point from the list in the dialog box.

3. Click on the part in the Graphics Display window to define the start point.

4. Select End Point from the list in the dialog box.

5. Click on the part in the Graphics Display window to define the end point.

PC-DMIS will fill up the necessary values in the List Box.