Current Help System: PC-DMIS Laser (View Core Help)

#### Filter Type: Point

This is only available for CMS sensors.

The Point Filter list lets you filter points along the scan line, much like the Column Sampling Rate for Perceptron sensors or the Inline Filter for Metris sensors. You can select a number from a scale of 1 to 10 (1 represents minimum filtering while 10 represents maximum filtering). If disabled, this acquires the complete data set without any filtering.

Example of Point Filtering Disabled

Example of Point Filtering of 5