Current Help System: PC-DMIS Laser (View Core Help)

### Laser Probe Toolbox: Laser Filtering Properties tab

Probe Toolbox - Laser Filtering Properties tab

The Filtering tab is useful when you want to filter the data as it is collected.

Because scanning methods with a portable device using a Perceptron laser differ from DCC machines, if you open the Auto Feature dialog box and are using a portable device with a Perceptron laser, this tab will be hidden.

The following filtering options are available from the list:

Filter Type: Only Available for Perceptron Sensors

- None - Filtering will not take place if you select 'None'. This is the default setting.

- Long Line

- Median

- Weighted Average

Filter Type: Only Available for Metris Sensors

- Inline

Filter Type: Only Available for CMS Sensors

- Point

- Stripe

Density Type: Only Available for Perceptron Sensors

- None - Density filtering will not take place if you select 'None'. This is the default setting.

- Intelligent Density Management (Contour V5 only)

- Column Sampling Rate