Current Help System: PC-DMIS Laser (View Core Help)

#### Auto Square Slot Paths

PC-DMIS must measure Auto Square slots at a 45 degree angle to the slot (see the illustrations below). Depending on the size of the slot, PC-DMIS takes one of these two paths.

Path 1: Small Slot - Measured with a single pass of the laser probe

Small square slots require a single pass of the laser probe’s stripe

Path 2: Large Slot - Measured with multiple passes of the laser probe

Large square slots require multiple passes of the laser probe’s stripe