Current Help System: PC-DMIS Laser (View Core Help)

### Laser Flush and Gap

Flush and Gap Auto Feature

To measure a Flush and Gap using a laser probe:

1. Access the Auto Features dialog box, and select Flush & Gap.

2. Do one of the following:

1. Click one time on the cad to give the flush and gap a location and vector. Then manually enter any remaining information.

2. Move the machine to the circle location using the Laser View tab of the Graphics Display Window. Next Click the Read Point from Position button. Then manually enter the any remaining information like the flush, gap, back off distance, bend radius, etc.

3. Manually enter all of the theoretical x, y, z, i, j, k, gap i, j, k, diameter, flush, gap, back off distance, bend radius, etc.

3. Enter the necessary information in the Probe Toolbox tabs. You will likely want to cycle through the Laser Scan, Laser Filtering, and Laser Clipping, properties tabs to enter the information.

4. Click the Test button if desired. Warning: The machine will now move!

5. Click the Create button and then Close.

More:

Flush and Gap Specific Parameters

Flush and Gap Command Mode Text