Current Help System: PC-DMIS Portable (View Core Help)

## Reporting Dimensions for Measured Points

PC-DMIS has a flag in the basic hit now that stores whether the probe has a shank vector. If it does not, then we display all three axes rather than just one. We also serialize this value because when we are reading in a part program, global_active_probe is not valid and we cannot check and set the flag using that mechanism.