Current Help System: PC-DMIS Portable (View Core Help)

## Calibrating a Romer Hard Probe

Calibration of a Romer Infinite probe is accomplished via the WinRDS software. PC-DMIS interfaces with WinRDS to acquire probe calibration data. Follow the steps found in the Arm Utilities User Guide document to calibrate your probe.

Perceptron Contour sensors are calibrated using the PC-DMIS Probe Utilities dialog box. See the "Calibrating a Perceptron Contour Sensor" topic for information on how this is done.