Current Help System: PC-DMIS Settings Editor (View Core Help)

### Distance To Closest Edge Tolerance In MM

This option is used during Edge Point Mode for portable devices or hard probes. The distance specified here determines the distance from the edge where guided mode will be initiated for completion of the edge point. See the Portable help file for more information on how this is used.

Entry Name: DistanceToClosestEdgeToleranceInMM

Entry Type: Real Number specifying distance in millimeters. Default value is 5.