Current Help System: PC-DMIS Settings Editor (View Core Help)

### UV Scan U Start

Defines the start location of the area on the scan surface in the U direction (approximate X Direction) that will be included as part of the UV Scan. For example, a value of .1 would begin scanning 10% of the way in the U direction.

Entry Name: UVScanUStart

Entry Type: Real Number specifying portion of the whole surface (1). Default value is 0.1.