Current Help System: PC-DMIS Settings Editor (View Core Help)

### DCC XYZ2_0

Provides the default "X" or "R" (radius) value for the for the end point of a line auto feature. The value will represent X value when the "Cartesian" value is set to TRUE (1), and R when it is set to FALSE (0). This value and the "DccXYZ2_1" and "DccXYZ2_2" values are used for Contact probes while the "Point2(XYZ)" values are used for Vision probes.

Entry Name: DccXYZ2_0

Entry Type: Real Number to specify the X or R value. Default value is 0.