Current Help System: PC-DMIS Settings Editor (View Core Help)

### Fly Mode

Fly Mode provides a way to move the probe around the part in a smooth, non-stopping motion. The Fly command can only be inserted before or after any feature in the part program and is used in conjunction with a Move Point command. Setting this option to TRUE (1) enables Fly Mode.

Entry Name: FlyMode

Entry Type: Whole Number to specify TRUE (1) or FALSE (0). Default value is 0.

See Also: FlyRadius