Current Help System: PC-DMIS Settings Editor (View Core Help)

### Slave High Threshold (0-3)

The Slave High Threshold values provide an upper limit (in the appropriate units) on the current temperature above which no further thermal compensation will be applied for the slave arm of a dual arm machine.

Entry Name: SlaveHighThreshold(0-3)

Entry Type: Character String specifying degrees in either Celsius or Fahrenheit. Default value is 0.0.

Number Key:

0 | X Axis
1 | Y Axis
2 | Z Axis
3 | Part