Current Help System: PC-DMIS Vision (View Core Help)

### Calibrate NC100 Video Probe

Now you will need to calibrate the angles used by your NC-100 Vision probe. An NC-100 video probe is the first optical probe available on the market that can be calibrated in multiple orientations.

To calibrate an NC-100 probe:

1. From the Probe Utilities dialog box specify the probe, extension and optical probe for your NC-100 system.

2. Click the Add Angles button. The Add New Angles dialog box appears.

3. Add any angles required by your part program. These angles should be normal to the part feature you will measure.

4. Click OK to return to the Probe Utilities dialog box.

5. Click Measure. The Measure Probe dialog box appears.

6. Select the DCC option button.

7. Select the Calibrate Tips option button from the Type of Operation area.

8. Select the polyhedral tool from the List of Available Tools list.

9. Click the Measure button. PC-DMIS will calibrate the probe positions you selected.

You've successfully calibrated your probe.