Current Help System: PC-DMIS Vision (View Core Help)

### Step 2: Home your System

Once you have started PC-DMIS Vision you are ready to home your system.

You need to home your system before proceeding in order to find the encoder’s zero position of the machine’s scales. Methods for homing may vary from system to system, although most DCC Vision systems will automatically home on startup. If you need additional information on homing your specific system, consult the documentation that came with your Vision machine.

Next Step...