Current Help System: PC-DMIS Vision (View Core Help)

## Calibrating the Vision Stage

The Vision Stage Calibration utility is used to generate and apply XYZ error correction factors on vision machines. The calibration process consists of one or more calibration runs and one or more verification runs for each axis. The average data of all calibration runs is used for verification and generation of the compensation file.

Note: This calibration, unlike the others, is NOT zoom cell specific. This is a machine level calibration.

Upon completion, a new compensation file will be created. The new compensation data will be applied the next time that PC-DMIS starts.

Note: Your portlock must be programmed with VCP counts in order to calibrate using the ASI compensation with the XY grid.

Continue with the following steps to complete the stage calibration process:

Step 1: Begin the Calibration Process

Step 2: Stage Calibration Setup - General tab

Step 3: Stage Calibration Setup - Standards tab

Step 4: Stage Calibration Setup - Report Information tab

Step 5: Running Stage Calibration

More:

Vision Stage Calibration Dialog Box Options