Current Help System: PC-DMIS Vision (View Core Help)

#### Step 2: Calibrate the Probe Tip Positions on a Sphere Calibration Tool

Now you will calibrate the two tip positions on a sphere calibration tool.

1. Select the two tips that you will use to establish the initial orientation of the Polyhedral Gage from the Active Tip List.

2. Click the Measure button on the Probe Utilities dialog box. The Measure Probe dialog box appears.

3. Select a calibration sphere from the List of Available Tools list.

4. Click Measure to calibrate the T1A0B0C0, T1A90B180C0 tips on a calibration sphere.

5. Follow the on-screen instructions.

Note: Even though you will use the polyhedral calibration tool in subsequent steps you should keep the sphere tool where it is on the CMM plate for further use in this procedure.

Next Step...