Current Help System: PC-DMIS Vision (View Core Help)

#### Square Slot/Gap and Flush Field Definition

Many of the definitions are already covered in the "Square Slot Field Definitions" topic in the "Creating Auto Features" section. The following definitions are added or changed when using a NC-100 video probe :

SHOWHITS = This is a toggle field. It toggles from YES to NO and determines if hits will be displayed with this feature.

SHOWALLPARAMS = This is a toggle field. It toggles from YES to NO as to displaying all the parameters on the feature.

ACTL_THICKNESS = This value indicates the keyed in offset thickness of the measured data. Positive or negative values can be used.

TOG2 = This field determines the fixed side of a Gap & Flush measurement. Only available on Gap & Flush.

THEO / = This value represents the theoretic feature location.

DEPTH = This value is editable and represents the depth of measurement on the fixed side of a Gap & Flush.

DEPTH2 = This values is editable and represents the depth of measurement on the moving side of a Gap & Flush.

See the "Common Auto Feature Dialog Box Options" topic in the "Creating Auto Features" section for general guidelines on measuring all Auto Feature types.