PC-Dmis 2010 MR3 Object Library | Send comments on this topic. | See Object Hierarchy Chart
FeatCmd Object Members
See Also Overview

Collapse All Expand All

# Public Methods

AddInputFeat | Appends to list of Input Features Adds a feature to set of input features used in constructed features.
AddInputFeatures | Appends an array of IDs to the list of Input Features
CalculateNominals | Recalculate the feature nominals This method recalculates feature nominals for a measured feature.
CountHits | Recount the hits for a measured feature Recounts the hits for a measured feature.
Evaluate | Evaluates the feature Forces an evaluation of a feature without executing it. This takes one parameter that specifies the type of feature evaluation to perform.
GenerateHits | Generates hits for measured features [Desc already exists]
GetCircMoveItem | Returns Point Data Object with interpolated circular move item data
GetData | Gets feature data relative to provided parameters [Desc already exists]
GetFormError | Returns Y14.5.1 Form error if applicable, else 0.0
GetHit | Returns Point Data Object with hit data Returns a PointData object with the values of the sample hit.
GetInputID | Gets ID of Input Feature
GetInputOffset | Gets Offset value for corresponding offset feature in constructed offset features Gets Offset value for corresponding offset feature in constructed offset features
GetPoint | Returns values for specified feature point type This method retrieves point information for individual objects.
GetPoints | Returns all Point Data Objects with hit data
GetSampleHit | Returns Point Data Object with sample hit data Returns a PointData object with the values of the sample hit.
GetSurfaceVectors | Gets Values of Surface Vectors for Auto Edge Feature This method gets the surface vectors of an angle hit function.
GetVector | Returns values for specified feature vector This method retrieves vector components of individual objects.
PutData | Puts feature data relative to provided parameters This function returns TRUE if the data was successfully retrieved from expression, FALSE otherwise.
PutPoint | Sets feature point data for specified point type Sets point information for individual objects.
PutSurfaceVectors | Sets Values of Surfave Vectors for Auto Edge Feature Sets the surface vectors for an angle hit object.
PutVector | Sets vector values for specified feature vector Sets vector components of individual objects.
RemoveInputFeat | Removes Constructed Feature Input Feature Removes the feature at the specified index position.
SetHit | Sets hit data of specified hit using part coordinates relative to the current alignment Sets the hit data of a specified hit. It uses the part coordinate system relative to the current alignment.
SetHit2 | Sets hit data of specified hit This method works just like the SetHit method; it sets the hit data of a specified hit, but it uses a specified coordinate system and alignment.
SetInputFeat | Sets Constructed Feature Input Feature Replaces the input feature at position Index in FeatCmd object's list of input features with ID.
SetInputOffset | Sets Offset value for coresponding offset feature in constructed offset features

# Public Properties

AlignWorkPlane | Read/Write: Workplane for Constructed Alignment Plane and Line Workplane value for constructed alignment planes and lines.
AutoCircularMove | Read/Write: Flag indicating if circular moves should be used during measurement Flag indicating whether circular moves should be used between hits.
AutoClearPlane | Read/Write: Flag indicating if clearance planes should automatically be used with the feature Flag indicating whether clearance planes should automatically be used with the feature.
AutoMove | Read/Write: Use Auto Move Setting Auto Move Flag.
AutoMoveDistance | Read/Write: Auto Move Distance Distance used in calculating auto move.
AutoPH9 | Read/Write: Flag indicating if the selected tip should be adjusted automatically Flag indicating if selected tip should be automatically adjusted during measurement of feature.
AutoReadPos | Read/Write: Auto Read Position Setting Auto Read Position Flag.
BestFitMathType | Read/Write: Type of math algorithm used to best fit the feature Value representing the best fit math algorithm to be used in calculating the measured feature values based on the measured hits. Possible values include the following.
Bound | Read/Write: Flag indicating whether object is bound or unbound Flag indicating whether or not feature is bound.
BoxLength | Read/Write: Auto High Point Box Length Box length value for auto high point.
BoxWidth | Read/Write: Auto High Point Box Width Box width value for auto high point.
CircularRadiusIn | Read/Write: Auto High Point Inner Circular Radius Inside circular radius value for auto high point.
CircularRadiusOut | Read/Write: Auto High Point Outer Circular Radius Outside circular radius value for auto high point.
CornerRadius | Read/Write: Auto Notch and Auto Square Slot Corner Radius Corner radius value for auto square slot and auto notch objects.
DCCFindNomsMode | Read/Write: Flag indicating whether measurement occurs in findnoms mode Indicates if the measurement mode for an auto feature should be done in find nominals mode or not.
DCCMeasureInMasterMode | Read/Write: Flag indicating whether measurement occurs in master mode Indicates if the measurement mode for an auto feature should be done in master mode or not.
Depth | Read/Write: Auto feature depth Gets or sets a depth value for a feature command.
Deviation | Read/Write: Auto Sphere Deviation Auto sphere deviation value.
DisplayConeAngle | Read/Write: Flag indicating whether angle or length is displayed for cone Flag indicating whether or not to display the angle of the cone. If this value is false, then the cone length is displayed.
EdgeMeasureOrder | Read/Write: Auto Edge Measure Order Measure order for edge points.
EdgeThickness | Read/Write: Auto Edge Thickness Thickness value for edge points.
EndAngle | Read/Write: Feature End Angle End Angle value.
EndAngle2 | Read/Write: End Angle 2 Second End Angle value.
FilterType | Read/Write: Filter Object Linear/Polar Setting Filter object filter type.
FindHole | Read/Write: Use Find Hole Routine Flag indicating whether or not to use the Find Hole routine. If this value is true, then the Find Hole routine is used.
GenericAlignMode | Read/Write: Generic Feature Alignment Dependence Value Generic alignment mode.
GenericDisplayMode | Read/Write: Generic Feature Diameter/Radius Display Type Generic display mode.
GenericType | Read/Write: Generic Feature Type Generic feature type.
HighPointSearchMode | Read/Write: Auto High Point Search Mode Search mode for auto high point.
ID | Read/Write: Feature ID Represents the ID of the feature.
Increment | Read/Write: Auto High Point Increment Value Increment value for auto high point.
Indent | Read/Write: Auto feature indent value Indent distance (used with sample hits).
Indent2 | Read/Write: Auto Feature Indent 2 Value Second indent distance (used with sample hits).
Indent3 | Read/Write: Auto Feature Indent 3 Value Third indent distance (used with sample hits).
InitHits | Read/Write: Initial Hits Number of initial sample hits.
Inner | Read/Write: Inside/Outside Feature Indicates whether the feature is a hole (inner) or a stud (outer).
InteriorHit | Read/Write: Flag indicating whether hits are exterior or interior hits Flag used to indicate type of hit for objects that can have interior/exterior hits.
Line3D | Read/Write: Flag indicating whether line is two dimensional or three dimensional Indicates whether the feature is a three dimensional line or a two dimensional line. A value of false indicates a two dimensional line.
ManualPrePosition | Read/Write: Manual PrePosition
MeasAngle | Read Only: Measured Angle Measured angle value.
MeasDiam | Read Only: Measured Diameter Measured diameter value.
MeasHeight | Read Only: Measured Height This property applies only to PC-DMIS commands that have a height field.
MeasLength | Read Only: Measured Length This property applies only to PC-DMIS commands that have a length field.
MeasMajorAxis | Read Only: Auto Ellipse Measured Major Axis Measured major axis length value (ellipse).
MeasMinorAxis | Read Only: Auto Ellipse Measured Minor Axis Measured minor axis length value (ellipse).
MeasPinDiam | Read Only: Measure Pin Diameter Measured pin diameter value.
MeasSmallLength | Read Only: Measured Small Length Measured shorter length value.
MeasureSlotWidth | Read/Write: Measure Slot Width Flag Flag indicating whether the slot width should be measured.
NumHits | Read/Write: Number of hits Represents the number of inputs in the feature.
NumHitsPerRow | Read/Write: Number of hits per row Represents the number of hits on each row of the feature.
NumRows | Read/Write: Number of rows Represents the number of rows in the feature.
Parent | Read Only: Parent Command Object Returns the parent Command object.
PermHits | Read/Write: Auto feature permanent hits Number of permanent sample hits.
Polar | Read/Write: Flag indicating whether polar coordinates are used Flag indicating whether polar coordinates are used on the feature. Usually defaults to false.
ReferenceID | Read/Write: Name of reference feature when reference type is feature ID of the feature to be used when the "ReferenceType" property is set to FEATREF_FEATURE. This property is used with measured lines or measured circles.
ReferenceType | Read/Write: Reference type for measured circles and lines Reference type used with measured circles and measured lines.
RMeasFeature | Read/Write: Relative Measure Feature ID of the feature to be used for relative measurement.
Spacer | Read/Write: Auto feature spacer Spacer distance (Usually used with sample hits).
StartAngle | Read/Write: Feature Start Angle Start Angle value.
StartAngle2 | Read/Write: Start Angle 2 Second Start Angle value.
Targets | Read Only: Returns the child Targets Collection Object of a vision feature
TheoAngle | Read/Write: Theoretical Angle Theoretical angle value.
TheoDiam | Read/Write: Theoretical Diameter Theoretical diameter value.
TheoHeight | Read/Write: Theoretical Height Theoretical height value.
TheoLength | Read/Write: Theoretical Length Theoretical length value.
TheoMajorAxis | Read/Write: Auto Ellipse Theoretical Major Axis Theoretical major axis length value (ellipse).
TheoMinorAxis | Read/Write: Auto Ellipse Theoretical Minor Axis Theoretical minor axis length value (ellipse).
TheoPinDiam | Read/Write: Theoretical Pin Diamter Theoretical pin diameter value.
TheoSmallLength | Read/Write: Theoretical Small Length Theoretical shorter length value.
Thickness | Read/Write: Auto feature thickness Sheet metal (material) thickness.
Tolerance | Read/Write: Auto High Point Tolerance Value Tolerance value for auto high point.
UsePin | Read/Write: Use Pin Vector Setting Indicates whether pin information should be used during measurement.
UseTheoValuesForBestfit | Read/Write: Use theo values to solve feature
VisionMag | Read/Write: Vision Feature Magnification
VisionTargetColor | Read/Write: Vision Feature Target Color
VisionTargetType | Read/Write: Vision Feature Target Type

# See Also

FeatCmd Overview

© Wilcox Associates, Inc. All Rights Reserved.

© 2010 All Rights Reserved.