PC-Dmis 2010 MR3 Object Library | Send comments on this topic. | See Object Hierarchy Chart
BasicScan Object Members
See Also Overview

Collapse All Expand All

# Public Methods

AddControlPoint | Adds a control point to the scan Adds a control point to a scan.
CreateBasicScan | Used for DCC and Manual Scans to cause creation of basic scan object This method creates a basic scan object.
GenerateScan | Generates the points for the scan
GetBoundaryConditionParams | Gets the boundary condition parameters
GetBoundaryPoint | Returns the boundary point specified by the index
GetControlPoint | Returns the control point specified by the index Returns the control point specified by the index.
GetFilterParams | Gets parameters used in filtering of scan data
GetHitParams | Gets parameters for the hit type used in the scan
GetHitTValue | Returns T deviation values for specified scansion hit
GetMethodParams | Gets the scan method parameters
GetMethodPointData | Gets scan points and vectors via pointdata objects This method is provided as a shortcut to getting these commonly used scan parameters all at once.
GetNomsParams | Gets the parameters used in finding of scan nominals
GetParams | Gets the basic scanning parameters of the scan This method is provided as a shortcut to getting commonly used scan parameters all at once.
RemoveControlPoint | Removes the control point at the specified index Removes a control point.
SetBoundaryConditionParams | Sets the boundary condition parameters Boolean value. Boolean returns true if the function succeeds, false if it fails.
SetBoundaryPoint | Sets the boundary point specified by the index paramter Sets a boundary point.
SetControlPoint | Sets the control point at the specified index Sets a control point at the specified index.
SetFilterParams | Sets parameters for filtering scan data This method is provided as a shortcut to set these commonly used scan parameters all at once.
SetHitParams | Sets parameters for the hit type used in the scan This method is provided as a shortcut to set these commonly used scan parameters all at once.
SetMethodParams | Sets the scan method parameters This method is provided as a shortcut to set these commonly used scan parameters all at once.
SetMethodPointData | Sets scan points and vectors via pointdata objects This method is provided as a shortcut to set these commonly used scan parameters all at once.
SetNomsParams | Sets the parameters used in finding of scan nominals This method is provided as a shortcut to set these commonly used scan parameters all at once.
SetParams | Sets the basic scanning parameters of the scan This method is provided as a shortcut to set these commonly used scan parameters all at once.

# Public Properties

AutoClearPlane | Read/Write: Boolean value indicating if auto clear planes should be used Determines whether auto clearance planes mode is on or off.
BoundaryCondition | Read/Write: Boundary Condition (Sphere, Plane Cross, Cone, etc. Represents the boundary condition type.
BoundaryConditionAxisV | Read/Write: Returns/Sets via point data object the boundary scan's axis vector Represents the boundary condition axis vector. This vector is used as the axis of the Cylindrical and Conical BoundaryConditions.
BoundaryConditionCenter | Read/Write: Returns/Sets via point data object a boundary scan's center point Represents the boundary condition center. This Point is used by all Boundary Conditions and is the location of the Boundary Condition.
BoundaryConditionEndApproach | Read/Write: Returns/Sets via point data object the end approach for a boundary scan Represents the boundary condition end approach vector. This vector is used by all Boundary Conditions and is the Approach Vector of the Probe as it crosses the Boundary condition.
BoundaryConditionPlaneV | Read/Write: Returns/Sets via point data object the boundary scan's plane vector Represents the boundary condition plane vector. This vector is the normal vector of the Plane used by the Plane and OldStyle Boundary Conditions.
BoundaryPointCount | Read/Write: Long value indicating the number of boundary points for patch scans Indicates the number of boundary points to used in a patch scan.
DisplayHits | Read/Write: Boolean value indicating whether hits should be displayed or not Determines whether hits of the scan are displayed in the Edit window or not.
Filter | Read/Write: Distance Filter Type Represents the filter type.
HitType | Read/Write: Scan Hit Type (Vector, Surface, Edge) Represents the type of hit to use.
Method | Read/Write: Scan Type Represents the method type for this scan.
MethodCutPlane | Read/Write: Returns/Sets via point data object the cut plane vector Represents the method’s cut plane vector.
MethodEnd | Read/Write: Returns/Sets via point data object the ending scan point Represents the scan’s end point.
MethodEndTouch | Read/Write: Returns/Sets via point data object the end touch vector Represents the method’s end touch vector.
MethodInitDir | Read/Write: Returns/Sets via point data object the initial scan direction vector Represents the method’s initial direction vector.
MethodInitTopSurf | Read/Write: Returns/Sets via point data object the initial top surface vector Represents the initial Surface Vector for the Edge method.
MethodInitTouch | Read/Write: Returns/Sets via point data object the initial touch vector Represents the method’s initial touch vector.
MethodStart | Read/Write: Returns/Sets via point data object the starting scan point Represents the scan’s start point.
NominalMode | Read/Write: Find cad nominals or use master data Represents how to determine the nominal values for this scan.
OperationMode | Read/Write: Scan Operation Mode Represents mode of operation of the scan.
SinglePoint | Read/Write: Returns/Sets Single Point Mode Flag Determines whether single point mode is on or off.

# See Also

BasicScan Overview | BasicScanCommand Property

© Wilcox Associates, Inc. All Rights Reserved.

© 2010 All Rights Reserved.