#### Placing Hits on a Feature

In many instances it is necessary to precisely position hits on a feature other than a plane. To do this:

1. Move the cursor close to the position where you wish to take the hits.

2. Hold down the left mouse button.

3. Move the probe towards the position where you want to take the hit. (the probe must be moved at least 1/8" on the screen).

4. Release the button.

PC-DMIS will "snap" the hit on the feature. PC-DMIS will locate the hit on the side of the feature where the cursor was positioned when you first held down the mouse.