### Calibrating the SCP600 Probe Changer

The process presented in these topics covers defining and calibrating the SP600 probe changer.

There are no inserts or extensions used for any of the slot positions.

A Renishaw SCP600 Stylus Change Rack

Important: The SCP600 Probe Changer MUST BE mounted on the machine table parallel to either the X or Y axis.
For mounting instructions, consult the documentation that came with your probe changer.

To Calibrate your SCP600 Probe Changer:

- Step 1 - Select the SCP600 Probe Changer

- Step 2 - Define the Mount Point

- Step 3 - Define the Number of Slots

- Step 4 - Prepare for Calibration

- Step 5 - Take the First Manual Hit

- Step 6 - Take the Second Manual Hit

- Step 7 - Review Calibration Results

###