## Constructing an Adjusted Filter

The Adjust Filter construction type lets you adjust scan data that was gathered while scanning around these standard geometric features:

- Sphere

- Cone

- Cylinder

Generally, you will perform these scans using an analog probe, such as an SP600. If you imagine a scan around the top quarter of a sphere, for example, you would ideally get points that lie within a plane that cuts through the sphere, like this:

| A - Scan Path

However, in reality, as the probe scans around the sphere it is physically impossible for all the points to remain inside the cut plane due to a natural rise and fall floating motion of the CMM.

The Adjust Filter construction can take the pre-existing scanned points and, using the known mathematical properties of the feature, can better compensate the points gathered during the measurement process, adjusting them to lie more within the cut plane. You use the Adjust Filter dialog box to do this. To access this dialog box, select Insert | Feature | Constructed | Adjust Filter from the menu bar.

Adjust Filter dialog box

Dialog Box Item | Description
Feature Type | This defines the primitive (simple geometric feature) being scanned. You can only select Sphere, Cone, or Cylinder.
Filter Type | This defines the type of filter to use. You can select Axial or Radial (used for Cone and Cylinder feature).
Feature Info | This lets you define the information about the feature. XYZ – The feature's nominal position. IJK – The feature's normal vector. Radius/Angle – This sets the Radius of the Sphere or Cylinder or the angle of the Cone.
Cut Plane Info | This area defines the location and vector of the cut plane. XYZ – Location of the cut plane IJK – Vector of the cut plane

To Adjust Scan Data:

To correctly adjust the data in the scan, you need to give enough information to mathematically define the feature.

1. Select the actual sphere, cone, or cylinder feature from the list of features in the Adjust Filter dialog box.

2. Select a pre-existing scan feature from the list. Generally your scanned feature will be a pre-existing linear closed scan. The scan must be of a sphere, cone, or cylinder.

3. Choose the feature type you scanned with the selected scan from the Feature Type list.

4. From the Filter Type list, choose the correct filter type for a Cone or Cylinder feature. The filter indicates how to compensate the data.

- If you are scanning perpendicular to the axis of the Cylinder or Cone, choose the Radial filter. This defines the circle that will be used to adjust the points.

- If you are scanning parallel to the feature's axis, choose the Axial filter. This defines a line that will be used to adjust the points.

5. Define the feature's nominal XYZ location by typing the values in the XYZ boxes.

6. Define the feature's normal vector by typing the values in the IJK boxes.

7. Define the feature's size by typing a value in the Radius or Angle box.

8. In the Cut Plane Info area, define the scan's cut plane. Once you specify all the nominal information for the scanned feature, you can create the construction.

9. Click Create. All the points are projected into the cut plane along the features theoretical definition (taking into account the known geometry) rather than a straight projection along the features normal vector.