#### Step 10 - Review Calibration Results

Select the Slots tab on the Probe Changer dialog box, and you will see that calibration information now exists for the location of each of the calibrated ports.

Probe Changer dialog box - Slots tab with calibration results

When viewing the results, some things to watch for are the position and spacing of the slots. For example, the ACR1 rack defined in this calibration process is aligned parallel to the Y axis of the CMM. The X values of the slots should be, within reason, nearly identical since all the slots are co-linear. Similarly, the Z values should also be nearly identical, since the slots are all at the same height. Finally, the Y values should be equally spaced, roughly 35mm apart. Any significant deviations from these expectations might be due to a bad hit.

Results During Part Program Execution

- During part program execution, probe entities that are added to each of the ports will be automatically picked up from that location whenever PC-DMIS executes a LOADPROBE command for that probe.

- The probe body will move to the mount point, then into the port, pushing the lid backwards.

- The key mechanism will automatically turn to dis-engage/engage, and it will load the new module and then continue measurement.