### Axes and Angle Offset

The offset area contains these boxes:

X Axis, Y Axis, and Z Axis boxes. These boxes set up the x, y, or z offset between parts, or patterns on the same part. These will offset the part by the entered distance each time the loop runs. The first offset is based on the part's origin.

The Angle box sets up the angular offset between parts, or patterns on the same part. The first offset is based on the part's origin. PC-DMIS offsets the part by the angle value each time the loop runs.

More:

Looping Offsets and Alignments