#### Step 5 – Take First Manual Hit

You will be prompted through the process of measuring two manual hits through a series of message boxes. Two hits are required to define the location of this rack in the machine’s workspace. Follow the prompts and take the needed hits as shown in the pictures for each hit.

The first manual hit is taken in the XY plane, on the vertical face in front of the rack on the left side of the port.

Prompt for the First Hit on the Front Face

PC-DMIS MESSAGE: Please take a hit on the black front face on the left side of port 1.

Using your machine's jog box, measure the first hit on the front face to the port, left of the opening. |

Next Step