### Calibrating the SP600 Probe Changer

The process presented in these documentation topics covers defining and calibrating the SP600 probe changer.

There are no inserts or extensions used for any of the slot positions.

A Renishaw SP600 Stylus Change Rack (SCR600)

Important: The SP600 Probe Changer DOES NOT need to be mounted on the machine table parallel to either the X or Y axis.
For mounting instructions, consult the documentation that came with your probe changer.

To Calibrate your SP600 Probe Changer:

- Step 1 - Select the SP600 Probe Changer

- Step 2 - Define the Mount Point

- Step 3 - Prepare for Calibration

- Step 4 - Take the First Manual Hit

- Step 5 - Take the Second Manual Hit

- Step 6 - Take the Third Manual Hit

- Step 7 - Review Calibration Results