#### Step 6 - Measure Port 1

You will be prompted through the process of measuring Port 1 (left-most port) and Port 8 (right-most port) through a series of message boxes. Follow the prompts and take the needed hits as shown in the pictures for each hit.

Take a Hit on the Back of Port 1

PC-DMIS MESSAGE: Please take a hit in the back of the circle for port 1. The hit should be taken in the middle just above the metal key.

Using your machine's jog box, measure the first hit on the back (arc) surface of Port 1 as shown in the image to the right. When you click OK you will be prompted to take the hit with the Execution Mode Options dialog box. |

Next Step