### Parameter Settings: NC-100 Parameters tab

Parameter Settings dialog box-NC-100 Parameters tab

The NC-100 Parameters tab only appears in the Parameter Settings dialog box if you have selected a NC-100 Video probe as your active probe. | The NC-100 Parameters tab allows you to change the parameters for the NC-100 Video Probe. These parameters are used to control the lighting, sizing etc. of the NC-100 vision area. If the values in the NC-100 tab are changed, then PC-DMIS inserts a new VIDEOSETUP command into the part program, and displays the cursor position in the Edit window. The Edit window command line for the VIDEOSETUP command reads:

VIDEOSETUP/GAIN = n, OFFSET = n, TOP = n, BOTTOM = n, WIDTH = n,YORIGIN = n,
YEND = n, LSEG = n, XSEG = n, YSEG = n

To edit information in the NC-100 Parameters tab:

1. Access the Parameter Settings dialog box (Edit | Preferences | Parameters).

2. Click on the NC-100 Parameters tab.

3. Select the value you want to change.

4. Type a new value.

5. Click Apply or OK.

The boxes contained in the NC-100 Parameters tab allow you to specify information that corresponds to settings on the NC-100 computer system See documentation from your NC-100 computer system for more detailed information on these settings.

More:

Gain

Offset Value

ROI Top

ROI Bottom

ROI Width

Y Origin

Y End

Long Segment

X Segment

Y Segment

Video Setup