### Type

Probe Changer dialog box-Type tab

Before calibration can take place, the probe changer type must be chosen. Select the type of probe changer from the Probe Changer drop-down list. After a change of probe changer type, PC-DMIS must be restarted.

The docking speed can be altered to fine tune the operation of the change cycle. Simply type a new percentage value to set the docking speed.

More:

Active Probe Changer

Number of Probe Changers

Probe Changer Type

Docking Speed