#### Machine Position

The Machine Position area of this dialog box allows you to indicate a safe location to which the CMM can move prior to each change cycle. Usually, this safe location is approximately two inches above and in front of the probe changer rack. However, you may find it necessary to move to some other location depending on the type of probe changer.

To change the values for the CMM Position:

1. Select the previous value of the X, Y, or Z box you want to change.

2. Type the correct value for the appropriate boxes or use the Read Machine button to insert the current location of the CMM.