#### Editing Boundary Points

Boundary points can be edited by double-clicking the number of the desired point in the ‘#’ column.

This will display the Edit Scan Item dialog box allowing you to edit the X, Y, Z values.

Edit Scan Item dialog boxes depicting Flip button and Point at Hole check box

The column widths of the Boundary Point list can be varied by changing the width of the list display column header. This is done by selecting the right or left edge of a column header with the left mouse button and pulling the edge to the desired size. The width of each list display is individually set and determined by the user. This information is saved in the INI file to be used each time the fields are changed.

Flip:

The Flip button is only available when editing a vector. Clicking this button flips the selected vector.

Point At Hole:

The Point At Hole check box only becomes available when you work with Section scans. It allows you to change a non-hole point to a hole point.

A hole point defines where a linear section scan jumps over a hole that's found in its path. After clicking the Cut Cad button PC-DMIS places hole points on either side of any hole that interrupts the section scan.

Hole points are defined with the letter "H" following the point number (For example 1H, 2H, 3H etc.). These points, like any boundary point, are added to both the Boundary Points list and on the part model in the Graphics Display window.

Note: The Point At Hole check box is only available for non-hole points that you need to change to hole points. If you have a hole point that needs to be changed to a non-hole point, delete the hole point and create a new non-hole point.