### Step 6 - Take Second Manual Hit

The second manual hit is taken in the Z direction, on the horizontal face on top of the rack to the left of the open port.

Prompt for the Second Hit on the Top

PC-DMIS MESSAGE: Please take a hit on the black top face on the left side of port 1.

Using your machine jog box, measure the second hit on the top flat plastic surface of the port, left of the opening. |

Next Step