## Inserting a Move Rotary Table Command

The Insert | Move | Move Rotary Table menu item allows you insert a MOVE/ROTAB command at the cursor's current location. The complete command line in the Edit window is

Command line in the Edit window:
MOVE/ROTAB,angle,DIRECTION

Direction = determines the direction of the table rotation. Available options are:

Clockwise: | Rotates the table in a clockwise direction until it reaches the angle entered in the Rotate Table Angle box.
Counterclockwise: | Rotates the table in a counterclockwise direction until it reaches the angle entered in the Rotate Table Angle box.
Shortest: | Rotates taking the shortest route (either Clockwise or Counterclockwise) until it reaches the angle entered in the Rotate Table Angle box.

Upon encountering this command, PC-DMIS will rotate the table to a position determined by whichever MOVE/ROTAB command is active.

Example: Consider a part program that has multiple different MOVE/ROTAB commands. If you click on a particular portion of the part program and select the Move Rotary Table menu option, PC-DMIS rotates the table to the position determined by whichever MOVE/ROTAB command is active at that point in the part program.

This menu option is only available if your portlock is configured for rotary tables.