Current Help System: PC-DMIS CMM (View Core Help)

## Defining Probes

The first step in CMM part programming is to define which probes will be used during the inspection process. A new part program must have a probe file created and/or loaded before the measurement process can begin. Little can be accomplished in a part program until you load the probe.

PC-DMIS supports a wide variety of probe types and calibration tools. It also offers a unique method for calibrating a Renishaw PH9 /PH10 wrist. The tools used to define your probe and to calibrate it are all within the Probe Utilities dialog box. To access this dialog box, select Insert | Hardware Definition | Probe from the menu bar.

For information on the various options in this dialog box, consult the "Understanding the Probe Utilities Dialog Box" topic in the PC-DMIS Core documentation.

Hint: You can also define your probe by using the Probe Wizard. Click this icon from the Wizards toolbar to access the PC-DMIS's Probe Wizard.

More:

Defining a Contact Probe

Defining Star Probes

Calibrating Probe Tips

SP600 Calibration Information

SP600 Calibration Procedures

Using Separate Deviations for Discrete and Scan Measurements