Current Help System: PC-DMIS CMM (View Core Help)

### Placing the Probe into Readouts and Hits Mode

Some interfaces require that you toggle between Readouts and Hits Modes since these modes must operate exclusively from each other. This is due to the operation of these interfaces being in either a receiving state (Hits Mode - waiting for a hit signal) or a sending state (Readouts Mode - sending probe location data to the Probe Readout window. An LK-RS232 interface is an example of this type of interface.

Icon | Description
| Readouts Mode | If you have an LK interface, you can use the Readouts Mode icon to places the probe into readouts mode.
| Hits Mode | If you have an LK interface, you can use the Hits Mode icon to places the probe into hits mode.