Current Help System: PC-DMIS Laser (View Core Help)

#### Cylinder Command Mode Text

CYL2 =FEAT/LASER/,CYL2=FEAT/CYLINDER,CARTESIAN,IN

THEO/<1.895,1.91,1>,<0,0,1>,1.895,7

ACTL/<1.895,1.91,1>,<0,0,1>,1.895,7

TARG/<1.895,1.91,1>,<0,0,1>

DEPTH=3

SHOW FEATURE PARAMETERS=YES

SURFACE=THEO_THICKNESS,1

MEASURE MODE=NOMINALS

RMEAS=NONE,NONE,NONE

AUTO WRIST=NO

GRAPHICAL ANALYSIS=NO

FEATURE LOCATOR=NO,NO,""

SHOW_LASER_PARAMETERS=YES

POINT CLOUD ID=DISABLED

SENSOR FREQUENCY=25,OVERSCAN=2,EXPOSURE=18

FILTER=NONE