Current Help System: PC-DMIS Laser (View Core Help)

#### CMS Sensors

Laser Sensor tab for the CMS probe

1. From the Hardware/Software area displays the corresponding CMS toolkit version in the Toolkit Version list.

2. Use the IP address and Port # boxes to define the IP address and of the CMS controller.

3. If desired, use the Beep level box to set the volume for beep sounds coming out of the CMS controller. It can accept any value from 0 to 100. 0 turns off the volume completely.

4. If desired, use the Logging area to generate text-based log files containing communication between PC-DMIS and the laser sensor during part program execution. The information sent to the log files includes scans, nominals of calculated features, and so on. These files are then used by technical support to resolve certain involving your laser sensor.

- Log Enabled - This check box enables or disables logging to the log files.

- Open Log Folder - This button opens up the folder where the log files are saved. For example, for PC-DMIS 2010 MR3, the folder content is located in C:\ProgramData\WAI\PC-DMIS\2010 MR3\NCSensorsLogs\

- Delete logged data at startup - If this is marked, PC-DMIS deletes the logged data files from the log folder whenever you create a new part program.

The Laser Sensor tab also displays the installed CMS Toolkit version.