Current Help System: PC-DMIS Laser (View Core Help)

#### Setting Boundary Points Using the CAD Data Method

PC-DMIS lets you select the boundary points by using surface CAD data.

When using CAD surface data:

1. Make sure that you have imported solid CAD data.

2. Select that the Draw Surfaces icon .

3. Select a boundary point by clicking on the desired location in the Graphics Display window. PC-DMIS highlights the selected surface and automatically updates the value of the currently selected Boundary point. PC-DMIS then moves the focus to the next boundary point (if any are available). For PATCH scans, PC-DMIS automatically adds an extra boundary point if the current point is the last point in the list.