Current Help System: PC-DMIS Laser (View Core Help)

### Laser Probe Toolbox: Position Probe tab

Probe Toolbox - Position Probe tab

The Position Probe tab allows you to select the current probe file and tip. It also displays the current probe location in the active alignment coordinates. You can double click the X, Y or Z values to edit them.

Be aware that if you edit the current probe location it will move the machine to the new coordinate. Use caution when using this capability because it will move your machinery without any notice.

If you don't see any information in the Probes and Probe Tips lists of the Probe Toolbox, you need to first define a probe. see the "Defining Hardware" section in the main PC-DMIS help file on how to do this.

While you can use this tab with all probe types (contact, laser, or optical), this help file only covers PC-DMIS Laser related items. For information about the toolbox as it relates to probes in general, see the "Using the Probe Toolbox" section in the main PC-DMIS help file.

More:

To Position Your Laser Probe

Laser Controls for Position Probe tab