This cylinder is identified by using the following values:

Center = Indent Center Point

Vector = Surface Vector

Radius = Spacer

This plane is identified by using the following values:

Center = Measured Edge Point

Vector = Measured Surface Vector

Current Help System: PC-DMIS Laser (View Core Help)

#### Edge Point Specific Parameters

Depth: This defines the depth to use when calculating the edge point. This corresponds to the blue graphical visualization in the Graphics Display window. A depth of 0 will cause this feature to be calculated at the surface plane height, using data found at the lowest possible depth from the surface plane. A depth of any other value will cause it to be calculated at that depth.

Spacer: This controls the size of the area PC-DMIS uses to calculate the feature normal. This corresponds to the purple graphical visualization in the Graphics Display window.

Indent: This lets you define the location of the area PC-DMIS uses to calculate the feature normal. This corresponds to the red graphical visualization in the Graphics Display window.

Sample Edge Point with Depth, Spacer, and Indent graphical visualizations used in the Graphics Display window

Notes on Graphical Analysis and Contour Feature Extraction of Edge Points

If you don't see some graphical analysis points computed to the edge plane, consider the following:

- Edge Line Points - All the edge line points on the reference plane returned by the feature extractor are displayed. For analysis, the edge line points are computed using the distance (Indent value) from the reference plane center (center of the circular surface area defined by the Spacer value) to the edge line.

- Reference Plane Points - If the Spacer value is 0.0 then the reference plane points are not displayed. If the Space value is not 0.0 then the reference plane points are extracted from the point cloud, applying the following rules using the plane statistical data returned by the Contour feature extractor:

- Rule 1: All points that are outside of an imaginary cylinder
  are discarded.

- Rule 2: All points with a distance from an imaginary plane
  greater than the maximum plane error value are discarded.

- Rule 3: If any remaining points are higher than the allowed number (19900), the points are uniformly reduced to the allowed value.

For analysis, each reference plane point is computed the distance from the reference plane and the measured surface plane.

The following two images show the Edge Point laser graphical analysis:

- Graphical Analysis Example - Side View

- Graphical Analysis Example - Top View