Current Help System: PC-DMIS Portable (View Core Help)

### Two Button Configuration

The two modes for a two button configuration are discussed below:

Measure Mode

The following Measure Mode functions are available for the buttons indicated above:

1: DONE - Press < 1 second.

1: ERASE last hit - Hold > 1 second.

1: OPEN DRO - Hold > 1 second when there is no hit in the buffer.

1: TOGGLE DRO - Hold > 1 second when the DRO is already open. XYZ <-> XYZT. The "T" value is displayed.

2: HIT POINT - Press < 1 second.

2: PULLED HIT -Press, pull back, release with 1 second. See "Using Pulled Hits for Probe Compensation"

2: SCAN - Press, hold > 1 second, drag.

A: Buttons indicated by a circle with a red arrow perform the same function.

Mouse Mode

The following Mouse Mode functions are available for the buttons indicated above:

1: Mouse RIGHT Button - Used for popup menus.

1: PAN - Press and hold on the CAD model.

2: Mouse LEFT Button - Used for screen selections.

A: Buttons indicated by a circle with a red arrow perform the same function.

Switching Between Mouse Mode and Measure Mode

To switch to Mouse Mode: Press and hold the take hit button and then quickly press the done button (within the first second).

To switch to Measure Mode: Move the cursor to the top of the screen and press the middle button (left mouse button).

To toggle from either mode:

1. Turn the "F" axis to the limit, then

2. Turn the "E" axis 90 degrees.